# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of lifeboat with necessary equipment p 1 /…**

**Publication reference:** **HUSRB/1903/34/0029-LB01**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | RIB (Rigid Inflatable Boat) for professional, cost-effective organization of sailing camps, trainings and competitions and overseeing smaller sailing dinghies.  Specification of the RIB:   * Length overall: 5,4 – 5,8 m * Max beam (B): 2,2 - 2,32 m * Displacement (G): 360-520 kg * Crew – min. 5 * Built-in fuel tank – 40-60 liter capacity * Vacuum infused fiberglass reinforced vinylester hull * Aluminium propeller * Non-skidding surfaces * Tachometer, hour meter, fuel gauge * Hypalon tube, 1.300 g/m2 density material * On the tube: rub rails, handrail chord * Complete steering system * Water drain tube * Carpeted seat for 2 persons with backrest * Built-in anchor locker * Battery * Cover * Position light * Bimini tent * Required sfaety equipment in EU countries and Serbia |  |  |  |
| **2** | Specification of the motor engine:  Complete Lean Burn 50 HP 4-stroke outboard engine |  |  |  |
| **3** | Trailer suitable for transport of the RIB on public roads.  Specification for trailer:   * Permissible total weight: max 1.300 kg * Width: 2,45 m * Length: 6,25 m * Length of transportable boat: max 6 m * Uniaxial * Equipped with brake system * With pull-out lamp holder * 12 V electrical system * 13-pin adapter * 13" or 14" C wheel + 1 spare wheel   The trailer has to have necessary documentation for registration in EU and Serbia. |  |  |  |